A B C D E F G H I L M N O P R S T U V W

## I

I2C_MASTER_GET_HS - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_MASTER_GET_I2CMTP - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_MASTER_GET_STATUS - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_MASTER_RESET - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_MASTER_SET_HS - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_MASTER_SET_I2CMTP - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_MASTER_STATUS - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_SLAVE_GET_I2CSADR - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_SLAVE_GET_STATUS - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_SLAVE_RESET - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2C_SLAVE_SET_I2CSADR - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
I2CDeviceID - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  I2C Option - I2C Device ID
I2CDisableSchmitt - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  I2C Option - Disable Schmitt trigger
I2cMaster - Interface in com.ftdi.j2xx.interfaces
I2cSlave - Interface in com.ftdi.j2xx.interfaces
I2CSlaveAddress - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  I2C Option - Slave Address
id - Variable in class com.ftdi.j2xx.D2xxManager.FtDeviceInfoListNode
  Reserve
init() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Device
  Init FT_4222_Device class and sync the chip status internally
init(int[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_Gpio
  Initialize the GPIO interface of the FT4222H.
init(int) - Method in class com.ftdi.j2xx.ft4222.FT_4222_I2c_Master
  Initialize the FT4222H as an I2C master with the requested I2C speed.
init() - Method in class com.ftdi.j2xx.ft4222.FT_4222_I2c_Slave
  Initialize FT4222H as an I2C slave.
init(int, int, int, int, byte) - Method in class com.ftdi.j2xx.ft4222.FT_4222_Spi_Master
  Initialize FT4222H as an SPI master.
init() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Spi_Slave
  Initialize FT4222H as SPI slave.
init(int[]) - Method in interface com.ftdi.j2xx.interfaces.Gpio
  Initialize the GPIO interface
init(int) - Method in interface com.ftdi.j2xx.interfaces.I2cMaster
  Initialize the device as I2C master with the requested I2C speed.
init() - Method in interface com.ftdi.j2xx.interfaces.I2cSlave
  Initialize the device as an I2C slave.
init(int, int, int, int, byte) - Method in interface com.ftdi.j2xx.interfaces.SpiMaster
  Initialize the device as an SPI master.
init() - Method in interface com.ftdi.j2xx.interfaces.SpiSlave
  Initialize the deivce as SPI slave.
InvertCTS - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - Invert CTS signal
InvertCTS - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - Invert CTS signal
InvertCTS - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - Invert CTS signal
InvertDCD - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - Invert DCD signal
InvertDCD - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - Invert DCD signal
InvertDCD - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - Invert DCD signal
InvertDSR - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - Invert DSR signal
InvertDSR - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - Invert DSR signal
InvertDSR - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - Invert DSR signal
InvertDTR - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - Invert DTR signal
InvertDTR - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - Invert DTR signal
InvertDTR - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - Invert DTR signal
InvertRI - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - Invert RI signal
InvertRI - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - Invert RI signal
InvertRI - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - Invert RI signal
InvertRTS - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - Invert RTS signal
InvertRTS - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - Invert RTS signal
InvertRTS - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - Invert RTS signal
InvertRXD - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - Invert RXD signal
InvertRXD - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - Invert RXD signal
InvertRXD - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - Invert RXD signal
InvertTXD - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - Invert TXD signal
InvertTXD - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - Invert TXD signal
InvertTXD - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - Invert TXD signal
IO_ERROR - Static variable in class com.ftdi.j2xx.protocol.SpiSlaveResponseEvent
  Response code from spi slave processor
iSerialNumber - Variable in class com.ftdi.j2xx.D2xxManager.FtDeviceInfoListNode
  iSerialNumber field on the USB Device Descriptor.
isFT4222Device() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Device
  Check if the device is FT4222 device
isFtDevice(UsbDevice) - Method in class com.ftdi.j2xx.D2xxManager
  This queries if a plugged-in USB device is a valid FT_Device
isOpen() - Method in class com.ftdi.j2xx.FT_Device
  Returns the open status of the device.

A B C D E F G H I L M N O P R S T U V W

About FTDI | FTDI Licence Terms